5.Write an assembly language program to swap two 8-bit data using 8085 processor.

LDA 0000

MOV B,A

LDA 0001

MOV C,A

STA 0003

MOV A,B

STA 0004

HLT